[image: ]For “Design” Flood Events ponding in the floodplain storage zones has been considered to have occurred from pre-storm precipitation
Key Reference Point Locations:
· Kempsey Traffic Bridge Gauge
· Smithtown Gauge
Flood Level in “m AHD”
Vertical black line scrolls across as time in simulation indicator
Floodwater Depth Indicator (m) above ground / river bed level


This particular flood event movie takes 1.00 minutes to play and simulates flood behaviour for 120hrs
The video animation will automatically play using the device (PC/Laptop) default media player program. The movie can be paused at any time by clicking on the play button
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